

Functional Safety Concept Lane Assistance

**Document Version: [Version]**

**Template Version 1.0, Released on 2017-06-21**



# Document history

**[Instructions: Fill in the date, version and description fields. You can fill out the Editor field with your name if you want to do so. Keep track of your editing as if this were a real world project.**

**For example, if this were your first draft or first submission, you might say version 1.0. If this is a second submission attempt, then you'd add a second line with a new date and version 2.0]**

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Editor | Description |
| 05/05/2019 | 0.1 | Maanadoona | First draft |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

# Table of Contents

**[Instructions: We have provided a table of contents. If you change the document structure, please update the table of contents accordingly. The table of contents should show each section of the document and page numbers or links. Most word processors can do this for you. In** [**Google Docs**](https://support.google.com/docs/answer/116338?co=GENIE.Platform%3DDesktop&hl=en)**, you can use headings for each section and then go to Insert > Table of Contents.** [**Microsoft Word**](https://support.microsoft.com/en-us/help/285059/how-to-create-a-table-of-contents-by-marking-text-in-word) **has similar capabilities]**

[Document history](#_1t3h5sf)

[Table of Contents](#_ktt3lgighckp)

[Purpose of the Functional Safety Concept](#_fulgh8sf1ocg)

[Inputs to the Functional Safety Analysis](#_757cx6xm46zb)

[Safety goals from the Hazard Analysis and Risk Assessment](#_pi1c1upmo8jt)

[Preliminary Architecture](#_s0p6ihti6jgk)

[Description of architecture elements](#_cqb49updinx4)

[Functional Safety Concept](#_mx8us8onanqo)

[Functional Safety Analysis](#_mtn6qbhgsr36)

[Functional Safety Requirements](#_frlc9y84ede8)

[Refinement of the System Architecture](#_74udkdvf7nod)

[Allocation of Functional Safety Requirements to Architecture Elements](#_g2lqf7kmbspk)

[Warning and Degradation Concept](#_4w6r8buy4lrp)

# Purpose of the Functional Safety Concept

**[Instructions: Answer what is the purpose of a functional safety concept?]**

Ultimate goal of functional safety is avoiding accidents by reducing risk to acceptable levels

# Inputs to the Functional Safety Concept

## Safety goals from the Hazard Analysis and Risk Assessment

**[Instructions:**

**REQUIRED:**

**Provide the lane departure warning and lane keeping assistance safety goals as discussed in the lessons and derived in the hazard analysis and risk assessment.**

**OPTIONAL:**


**If you expanded the hazard analysis and risk assessment to include other safety goals, include them here.**

**]**

|  |  |
| --- | --- |
| **ID** | **Safety Goal** |
| Safety\_Goal\_01 | 1. The oscillating steering torque from the lane departure warning function shall be limited |
| Safety\_Goal\_02 | 1. The lane keeping assistance function shall be time limited, and the additional steering torque shall end after a given time interval so that the driver cannot misuse the system for autonomous driving. |
| Safety\_Goal\_03 | The LDW indication shall indicate the direction correctly |
| Safety\_Goal\_04 | The lane keeping assistance function shall indicate the it's malfunction. |

## Preliminary Architecture

**[Instructions: Provide a preliminary architecture for the lane assistance item. Hint: See Lesson 3: Item Definition]**



### Description of architecture elements

**[Instructions: Provide a description for each of the item elements; what is each element's purpose in the lane assistance item? ]**

|  |  |
| --- | --- |
| **Element** | **Description** |
| Camera Sensor | The Camera Sensor reads in images from the road. |
| Camera Sensor ECU | The Camera Sensor ECU identifies when the vehicle has accidentally departed its lane, and sends the appropriate messages to the Car Display ECU and the Electronic Power Steering ECU. |
| Car Display | Indicate the information of camera |
| Car Display ECU | Controller to show the Warning and status of Lane Departure Assistance and Lane Keeping Assistance. |
| Driver Steering Torque Sensor | Measure the torque of steering wheel |
| Electronic Power Steering ECU | Device to control and sense the motor actuator |
| Motor | Actuator for applying the torque to the steering wheel |

# Functional Safety Concept

The functional safety concept consists of:

* Functional safety analysis
* Functional safety requirements
* Functional safety architecture
* Warning and degradation concept

## Functional Safety Analysis

**[Instructions: Fill in the functional safety analysis table below.]**

|  |  |  |  |
| --- | --- | --- | --- |
| **Malfunction ID** | **Main Function of the Item Related to Safety Goal Violations** | **Guidewords (NO, WRONG, EARLY, LATE, MORE, LESS)** | **Resulting Malfunction** |
| Malfunction\_01 | Lane Departure Warning (LDW) function shall apply an oscillating steering torque to provide the driver a haptic feedback | MORE | The Lane Departure Warning function applies an oscillating torque with very high torque amplitude (above limit) |
| Malfunction\_02 | Lane Departure Warning (LDW) function shall apply an oscillating steering torque to provide the driver a haptic feedback | MORE | The Lane Departure Warning function applies an oscillating torque with very high torque frequency (above limit) |
| Malfunction\_03 | Lane Keeping Assistance (LKA) function shall apply the steering torque when active in order to stay in ego lane | NO | The lane keeping assistance function is not limited in time duration which leads to misuse as an autonomous driving function. |
| Malfunction\_04 | Lane Departure Warning (LDW) function shall receive the signal from camera sensor to decide the direction. | WRONG | The Lane Departure Warning function is deactivated when the camera sesor is not woking |
| Malfunction\_05 | Lane Keeping Assistance (LKA) function shall receive the signal from camera sensor to keep the lane. | WRONG | The Keeping Assistance function is deactivated when the camera sesor is not woking |

## Functional Safety Requirements

**[Instructions: Fill in the functional safety requirements for the lane departure warning ]**

Lane Departure Warning (LDW) Requirements:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Safe State** |
| Functional  Safety  Requirement  01-01 | The Lane Departure Warning item shall ensure that the lane departure oscillating torque amplitude is below Max\_Torque\_Amplitude. | C | 50 ms | Vibration torque amplitude below Max\_Torque\_Amplitude. |
| Functional  Safety  Requirement  01-02 | The Lane Departure Warning item shall ensure that the lane departure oscillating torque frequency is below Max\_Torque\_Frequency. | C | 50 ms | Vibration frequency is below Max\_Torque\_Frequency. |
| Functional  Safety  Requirement  01-03 | The Lane Departure Warning function is deactivated when the camera sesor is not woking | QM | 50 ms | Function is deactivated. |

Lane Departure Warning (LDW) Verification and Validation Acceptance Criteria:

|  |  |  |
| --- | --- | --- |
| **ID** | **Validation Acceptance**  **Criteria and Method** | **Verification Acceptance**  **Criteria and Method** |
| Functional  Safety  Requirement  01-01 | Validate Max\_Torque\_Amplitude chosen is high enough to be detected by a driver while low enough not to cause loss of steering | Verify the system does turn off if the Lane Departure Warning exceeded Max\_Torque\_Amplitude. |
| Functional  Safety  Requirement  01-02 | Validate Max\_Torque\_Frequency chosen is adequate to be detected by the driver and not cause the loss of steering. | Verify the system does turn off if the Lane Departure Warning exceeded Max\_Torque\_Frequency. |
| Functional  Safety  Requirement  01-03 | Validate Lane Departure Warning is off when the camera sensor give the wrong signal. | Verify the Lane Departure Warning is deactivated when the camera sensor is wrong. |

**[Instructions: Fill in the functional safety requirements for the lane keeping assistance]**

Lane Keeping Assistance (LKA) Requirements:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **ASIL** | **Fault Tolerant Time Interval** | **Safe State** |
| Functional  Safety  Requirement  02-01 | The electronic power steering ECU shall ensure that the Lane Keeping Assistance torque is applied only Max\_Duration. | B | 500 ms | Lane Keeping Assistance torque is zero. |
| Functional  Safety  Requirement  02-02 | The Keeping Assistance function is deactivated when the camera sesor is not woking | A | 50 ms | Function is deactivated. |

Lane Keeping Assistance (LKA) Verification and Validation Acceptance Criteria:

|  |  |  |
| --- | --- | --- |
| **ID** | **Validation Acceptance**  **Criteria and Method** | **Verification Acceptance**  **Criteria and Method** |
| Functional  Safety  Requirement  02-01 | Validate the Max\_Duration chosen not allow the driver to use the car as self-driving car. | Verify the system does deactivate if the Lane Keeping Assistance torque application exceeded Max\_Duration. |
| Functional  Safety  Requirement  02-02 | Validate the Lane Keeping assistance shall be deactivated when the camera sensor is broken. | Verify the Lane Keeping Assistance is deactivated if the camera sensor is not working. |

## Refinement of the System Architecture

**[Instructions: Include the refined system architecture. Hint: The refined system architecture should include the system architecture from the end of the functional safety lesson including all of the ASIL labels.]**



## Allocation of Functional Safety Requirements to Architecture Elements

**[Instructions: Mark which element or elements are responsible for meeting the functional safety requirement. Hint: Only one ECU is responsible for meeting all of the requirements.]**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Functional Safety Requirement** | **Electronic Power Steering ECU** | **Camera ECU** | **Car Display ECU** |
| Functional  Safety  Requirement  01-01 | The Lane Departure Warning item shall ensure that the lane departure oscillating torque amplitude is below Max\_Torque\_Amplitude. | **X** |  |  |
| Functional  Safety  Requirement  01-02 | The Lane Departure Warning item shall ensure that the lane departure oscillating torque frequency is below Max\_Torque\_Frequency. | **X** |  |  |
| Functional  Safety  Requirement  01-03 | The Lane Departure Warning function is deactivated when the camera sesor is not woking |  | **X** |  |
| Functional  Safety  Requirement  02-01 | The electronic power steering ECU shall ensure that the Lane Keeping Assistance torque is applied only Max\_Duration. | **X** |  |  |
| Functional  Safety  Requirement  02-02 | The Keeping Assistance function is deactivated when the camera sesor is not woking |  | **X** |  |

## Warning and Degradation Concept

**[Instructions: Fill in the warning and degradation concept.]**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **ID** | **Degradation Mode** | **Trigger for Degradation Mode** | **Safe State invoked?** | **Driver Warning** |
| WDC-01 | Turn off Lane Departure Warning functionality | Malfunction\_01,  Malfunction\_02,  Malfunction\_04 | Yes | Lane Departure Warning Malfunction Warning on Car Display |
| WDC-02 | Turn off Lane Keeping Assistance functionality | Malfunction\_03,  Malfunction\_05 | Yes | Lane Keeping Assistance Malfunction Warning on Car Display |